LABEL MACHINE SPECS

( TAL-750HD) http://www.take-a-label.com/tal-750hd/
According to the manufacturer:
The machine we now have does not require a gap between labels but can handle a gap of 1/8 inch and is also fine with the 5/16 inch gap that is sited on the digital proof you emailed us. Also, the machine can handle widths of up to 7.5 inches.